**Thoughts**

Should use 10-11 AWG cable to connect power between heating boards

Heating boards contain nothing but connector and track. Keep track density constant. Connect heating boards in sequency, don’t exceed 8A draw (should be roughly 2A per board).